I set the BLOCKLEN to 2 \*\*10

The spectrum of the output signal is similar to the input spectrum, however, the wave graph is smaller than the input one, it is because of the butter filer.